Fichier
. File -> Project -> Set project to current file
Composant
. Assign -> Device -> Show NOT only fastest speed grades -> Device Family FLEX10K -> Devices EPF10K20RC240-4
Synthese
. Max+plusII -> Compiler -> Processing -> Design Doctor -> Start
Simulation
. File -> New -> Waveform Editor File - > Save (SCF File)
Signaux a visualiser + Initialisation
. Node -> Enter Nodes from SNF -> List
. File -> End time
Simulation Run
. File -> Project -> Save, Compile and Simulation : Start + Open SCF
Implementation (Affectation des broches) + Compilation 
. Assign -> Pin/Location/Chip
. POF 
. JTAG -> Multi-Device JTAG Chain
. Device Name EPF10K20
. Select Programming File toto.sof
. Add
. Detect JTAG Chain Info
. OK
. Configure

. Attention : l'extension .scf n'apparait pas sous l'explorer de Windows